# Parameters for rigid deformation (tx, ty, tz, rx, ry, rz)
Transformation_parameters:
0,0,0,0,0,0
1,2,-3.5,-3.5,-2,4.5
3,-0.5,-4.25,3.75,-2,4.25
1,2,1.5,-0.75,-3.5,-3
-0.75,0.5,-2,-4,-3.25,-3
-0.5,3,2.5,1.75,-0.5,-3.5

# Convention of rotation (any combination of XYZ axis)
Rotation_convention: XYZ

# Parameters computation:
# 0: Each line of parameters represent the actual deformation in comparison with the reference position
# 1: Each line of parameters represent the deformation with the previous position. 
Transformation_mode: 0
